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Diesel Meister Fuel Dispensing Catalogue
DIESEL-MEISTER by STT Engineering Solutions
Commercial fuel dispensing equipment and accessories
For fleet yards, farms, construction sites and industrial facilities. Diesel-Meister by STT Engineering Solutions offers a fuel dispensing enquiry range, with equipment selection and final configurations confirmed on quotation.
DRIVING INDUSTRY FORWARD
info@stteng.co.zawww.stteng.co.za7 Lathe Street, Isando, GautengWhatsApp and landline numbers to be advised



Equipment selection
Select equipment to suit the fuel, site conditions and required delivery rate. Availability, supplier arrangements and any required certification are confirmed for the quoted equipment.


Fuel dispensing range
Choose equipment around the required filling rate, fuel type, available power and level of transaction control. The range below provides a starting point for an STT quotation.
	Equipment category
	Typical enquiry
	Selection details

	Mechanical dispensers
	Fleet and site refuelling
	60 L/min and 80 L/min categories; one hose and one product

	Electronic retail dispensers
	Metered dispensing with electronic displays
	Confirm model, hose count, products and control system

	Transfer pumps and kits
	Mobile or fixed tank transfer
	Specify power supply, flow, suction conditions and fuel

	Fuel management systems
	Authorised users and transaction records
	Confirm dispenser interface and reporting requirements

	Nozzles and flowmeters
	Fuel delivery and volume measurement
	Match fuel, flow rate, inlet thread and meter range

	Hoses and accessories
	Complete the dispensing assembly
	Specify length, diameter, connections and installation


Electronic dispensers and transfer equipment
Electronic dispensers and transfer kits are selected to suit the application. Specify the fuel, available power, delivery rate and transaction control requirements so STT can confirm a suitable configuration.
Complete the installation
A dispensing assembly may include a pump, meter, compatible filter, fuel hose, nozzle and isolation fittings. Fuel management, breakaways and hose reels depend on the chosen equipment and site requirements. Confirm the included items on the quotation.


Mechanical fuel dispenser
The stainless steel enclosure and mechanical register provide a starting point for commercial refuelling enquiries.
	Parameter
	Published reference

	Configuration
	1 hose and 1 product

	Flow rate
	80–85 L/min

	Measurement accuracy
	±0.3% as published by EHAD

	Body material
	Stainless steel 304

	Power supply
	AC 220 V, −15% to +10%; 50/60 Hz ±1 Hz

	Communication
	None listed

	Package dimensions
	450 × 450 × 1320 mm

	Gross weight
	130 kg


Package dimensions describe shipping packaging, not an installation envelope. Obtain the equipment drawing before positioning the unit.
Mechanical dispenser options
A 60 L/min mechanical dispenser option can be specified on enquiry. Confirm the model, operating conditions and supplied accessories on the quotation.
Details to confirm before ordering
Confirm approved fuel, actual delivery rate at the site, inlet and outlet connections, hose and nozzle specification, power connection and installation dimensions. Operating temperature limits and totalizer capacity must be confirmed for the selected model.


Accessories and quotation enquiries
Select each accessory to match the approved fuel and the operating flow and pressure of the complete system. Connection sizes and thread types must be confirmed together.
	Accessory
	Information required for selection

	Automatic or manual nozzle
	Fuel, delivery rate, spout size and inlet connection

	Mechanical or digital flowmeter
	Flow range, accuracy requirement and connections

	Fuel hose and reel
	Fuel compatibility, bore, length, pressure and fittings

	Filter assembly
	Fuel type, rated flow, element and water separation needs

	Breakaway and swivel
	Flow rating, connection size and dispenser compatibility

	Fuel management equipment
	Users, vehicles, authorisation and reporting requirements


Send us your requirements
Tell us the fuel type, tank arrangement, required litres per minute, approximate daily volume and available power. Include suction height, pipe length, hose reach, number of dispensing points and whether you need user identification or transaction reports.
For a replacement, send the existing model, nameplate photograph, connection sizes and installation photographs. We will use these details to prepare the equipment specification and quotation.
Contact STT Engineering Solutions
Diesel-Meister fuel dispensing enquiriesinfo@stteng.co.zawww.stteng.co.za7 Lathe Street, Isando, GautengWhatsApp and landline numbers to be advised
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